Fish was made vertical at the start of laps.

Encoder looped from 255 to 0 to 1023 and 755 and then back to 1023 and 0 to 255.

The initial files are extra in one SD card as we forgot to remove that after the system test right before packing the fish.

Sometimes SD card starts after a few seconds to not all data is synchronized with time but has a constant phase difference